IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [VersionGUID: afda6e5d-1ca2-475a-b745-dff31ce6d0f8, NumberOfSaves: 84]"
Description: "CoordinateReference [CoordinateBase: Project Base Point, ProjectSite: Default Site]"
File name: "ApartmentBlock.ifc"
Time stamp: "2025-09-24T12:58:44+02:00"
Preprocessor: "IfcOpenShell 0.8.3-post1"
Originating system: "Bonsai 0.8.3-post1"
Application: "Autodesk Revit 2024 (ENG)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENG)"
Application: "Bonsai" version "0.8.3" identifier "Bonsai-0.8.3" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

People and organizations
  Person "rcabreraDLB7V" of Organization (no name given)
  Owner history of Person "rcabreraDLB7V" of Organization (no name given) | application "Autodesk Revit 2024 (ENG)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENG)" | change NOCHANGE | created 1707906996 (2024-02-14T10:36:36Z)
  Owner history of Person "rcabreraDLB7V" of Organization (no name given) | application "Bonsai" version "0.8.3" identifier "Bonsai-0.8.3" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org") | state READWRITE | change ADDED | created 1758706133 (2025-09-24T09:28:53Z) | last modified 1758706133 (2025-09-24T09:28:53Z) by Person "rcabreraDLB7V" of Organization (no name given) with "Bonsai" version "0.8.3" identifier "Bonsai-0.8.3" by Organization "IfcOpenShell" id "IfcOpenShell" description "IfcOpenShell is an open source software library that helps users and software developers to work with IFC data." (roles: "CONTRIBUTOR"; telecom address "WEBPAGE": web page "https://ifcopenshell.org")

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  AREADENSITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Garage" | long name "Garage" | object type "Level:8mm Head" | elevation -250.
        contains 49 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm" | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:480769" | material: "Default Floor" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          18 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:482481", "Basic Wall:Retaining - 300mm Concrete:482482", "Basic Wall:Retaining - 300mm Concrete:580630" (+15 more) | material: "Concrete, Cast In Situ" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCSTAIR | type IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | object type "Assembled Stair:190mm max riser 250mm going" | names: "Assembled Stair:Stair:486954", "Assembled Stair:Stair:590974", "Assembled Stair:Stair:592494" | parts: 30 IFCMEMBER, 6 IFCRAILING, 3 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          8 x IFCWALL | type IFCWALLTYPE "Basic Wall:Garage Wall" | object type "Basic Wall:Garage Wall" | names: "Basic Wall:Garage Wall:501839", "Basic Wall:Garage Wall:502002", "Basic Wall:Garage Wall:502077" (+5 more) | material: constituents "Basic Wall:Garage Wall" ("Asphalt, Bitumen": "Asphalt, Bitumen", "Air": "Air", "Concrete, Cast In Situ": "Concrete, Cast In Situ") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          19 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:580634", "Basic Wall:Generic - 200mm:580635", "Basic Wall:Generic - 200mm:580636" (+16 more) | material: "Default Wall" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "0 - Ground Floor" | long name "0 - Ground Floor" | object type "Level:8mm Head" | elevation 0.
        contains 88 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm" | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:480757" | material: "Default Floor" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          18 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:480971", "Basic Wall:Retaining - 300mm Concrete:480972", "Basic Wall:Retaining - 300mm Concrete:580593" (+15 more) | material: "Concrete, Cast In Situ" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCSTAIR | type IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | object type "Assembled Stair:190mm max riser 250mm going" | names: "Assembled Stair:Stair:493113", "Assembled Stair:Stair:591105", "Assembled Stair:Stair:592559" | parts: 30 IFCMEMBER, 6 IFCRAILING, 3 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          8 x IFCWALL | type IFCWALLTYPE "Basic Wall:Exterior - Brick on Mtl. Stud_63cm" | object type "Basic Wall:Exterior - Brick on Mtl. Stud_63cm" | names: "Basic Wall:Exterior - Brick on Mtl. Stud_63cm:502575", "Basic Wall:Exterior - Brick on Mtl. Stud_63cm:502946", "Basic Wall:Exterior - Brick on Mtl. Stud_63cm:503015" (+5 more) | material: constituents "Basic Wall:Exterior - Brick on Mtl. Stud_63cm" ("Brick, Common(1)": "Brick, Common(1)", "Air": "Air", "Concrete Masonry Units": "Concrete Masonry Units", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          19 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:580597", "Basic Wall:Generic - 200mm:580598", "Basic Wall:Generic - 200mm:580599" (+16 more) | material: "Default Wall" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCDOOR | type IFCDOORTYPE "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass" | object type "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass" | DOOR | names: "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605218", "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:615069", "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:620268" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          6 x IFCDOOR | type IFCDOORTYPE "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass" | object type "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass" | DOOR | names: "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605751", "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:615603", "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:618962" (+3 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          3 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-30:Type 1" | object type "Jansen_Janisol-C4_fix_TL_Family-30:Type 1" | WINDOW | names: "Jansen_Janisol-C4_fix_TL_Family-30:Type 1:610414", "Jansen_Janisol-C4_fix_TL_Family-30:Type 1:610647", "Jansen_Janisol-C4_fix_TL_Family-30:Type 1:615013" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | object type "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | names: "Jansen_Janisol-C4_fix_TL_Family-10:Type 1:614611" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:615139" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:615259", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:615357", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:615899" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | object type "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | WINDOW | names: "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:615403", "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:615470" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | object type "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | WINDOW | names: "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:615478" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          5 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-30:Type 2" | object type "Jansen_Janisol-C4_fix_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-C4_fix_TL_Family-30:Type 2:615973", "Jansen_Janisol-C4_fix_TL_Family-30:Type 2:616843", "Jansen_Janisol-C4_fix_TL_Family-30:Type 2:616893" (+2 more) | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | DOOR | names: "M_Single-Flush:0915 x 2134mm:616505" | material: constituents ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | object type "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | names: "Jansen_Janisol-C4_fix_TL_Family-10:Type 1:617289" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | object type "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | WINDOW | names: "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:617926" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-30:Type 2" | object type "Jansen_Janisol-C4_fix_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-C4_fix_TL_Family-30:Type 2:618466", "Jansen_Janisol-C4_fix_TL_Family-30:Type 2:619912", "Jansen_Janisol-C4_fix_TL_Family-30:Type 2:619999" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | object type "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | WINDOW | names: "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:619201" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | object type "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | names: "Jansen_Janisol-C4_fix_TL_Family-10:Type 1:620536", "Jansen_Janisol-C4_fix_TL_Family-10:Type 1:620877" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | object type "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | names: "Jansen_Janisol-C4_fix_TL_Family-10:Type 1:620925", "Jansen_Janisol-C4_fix_TL_Family-10:Type 1:621391" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | object type "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | names: "Jansen_Janisol-C4_fix_TL_Family-10:Type 1:621112", "Jansen_Janisol-C4_fix_TL_Family-10:Type 1:621120" | material: constituents ("Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Storefront- meier_Garage" | object type "Curtain Wall:Storefront- meier_Garage" | names: "Curtain Wall:Storefront- meier_Garage:621515" | parts: 4 IFCMEMBER, 1 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
      IFCBUILDINGSTOREY "1 - First Floor" | long name "1 - First Floor" | object type "Level:8mm Head" | elevation 350.000000000035
        contains 109 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm" | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:355015" | material: "Default Floor" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          10 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 630mm-Render" | object type "Basic Wall:Generic - 630mm-Render" | names: "Basic Wall:Generic - 630mm-Render:356060", "Basic Wall:Generic - 630mm-Render:356102", "Basic Wall:Generic - 630mm-Render:356167" (+7 more) | material: constituents "Basic Wall:Generic - 630mm-Render" ("Render Material 240-240-240": "Render Material 240-240-240", "EIFS, Exterior Insulation": "EIFS, Exterior Insulation", "Concrete Masonry Units": "Concrete Masonry Units", "Render Material 240-240-240": "Render Material 240-240-240") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:396075", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:423686" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          5 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:397507", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:423360", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:424174" (+2 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423067", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:597443", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:597512" (+3 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423620", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:424065", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:602218" (+5 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Interior - Blockwork 190" | object type "Basic Wall:Interior - Blockwork 190" | names: "Basic Wall:Interior - Blockwork 190:433140", "Basic Wall:Interior - Blockwork 190:433141" | material: constituents "Basic Wall:Interior - Blockwork 190" ("Gypsum Wall Board": "Gypsum Wall Board", "Concrete Masonry Units": "Concrete Masonry Units", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0864 x 2134mm" | object type "M_Single-Flush:0864 x 2134mm" | DOOR | names: "M_Single-Flush:0864 x 2134mm:433302" | material: constituents ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:443514" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCSTAIR | type IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | object type "Assembled Stair:190mm max riser 250mm going" | names: "Assembled Stair:Stair:496383", "Assembled Stair:Stair:591250", "Assembled Stair:Stair:592624" | parts: 30 IFCMEMBER, 6 IFCRAILING, 3 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          3 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Storefront- meier" | object type "Curtain Wall:Storefront- meier" | names: "Curtain Wall:Storefront- meier:504174", "Curtain Wall:Storefront- meier:595921", "Curtain Wall:Storefront- meier:596200" | parts: 86 IFCMEMBER, 32 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_EnvironmentalImpactIndicators
          18 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:505319", "Basic Wall:Retaining - 300mm Concrete:505358", "Basic Wall:Retaining - 300mm Concrete:505420" (+15 more) | material: "Concrete, Cast In Situ" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          28 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:505673", "Basic Wall:Generic - 200mm:505758", "Basic Wall:Generic - 200mm:505894" (+25 more) | material: "Default Wall" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:597318", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598015", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598727" (+4 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598911", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:602899" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:599313" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599725" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:599740", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602029" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601471" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602615", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602802", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602980" (+1 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604423" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604531" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604544" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
      IFCBUILDINGSTOREY "2 - Second Floor" | long name "2 - Second Floor" | object type "Level:8mm Head" | elevation 650.
        contains 106 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm" | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:358327" | material: "Default Floor" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          10 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 630mm-Render" | object type "Basic Wall:Generic - 630mm-Render" | names: "Basic Wall:Generic - 630mm-Render:358336", "Basic Wall:Generic - 630mm-Render:358337", "Basic Wall:Generic - 630mm-Render:358338" (+7 more) | material: constituents "Basic Wall:Generic - 630mm-Render" ("Render Material 240-240-240": "Render Material 240-240-240", "EIFS, Exterior Insulation": "EIFS, Exterior Insulation", "Concrete Masonry Units": "Concrete Masonry Units", "Render Material 240-240-240": "Render Material 240-240-240") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:396342", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:423935" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          5 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:397798", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:423933", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:424372" (+2 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423285", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:598212", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:598213" (+3 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423934", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:424371", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:602521" (+5 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Interior - Blockwork 190" | object type "Basic Wall:Interior - Blockwork 190" | names: "Basic Wall:Interior - Blockwork 190:433277", "Basic Wall:Interior - Blockwork 190:433278" | material: constituents "Basic Wall:Interior - Blockwork 190" ("Gypsum Wall Board": "Gypsum Wall Board", "Concrete Masonry Units": "Concrete Masonry Units", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0864 x 2134mm" | object type "M_Single-Flush:0864 x 2134mm" | DOOR | names: "M_Single-Flush:0864 x 2134mm:433490" | material: constituents ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:443700" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCSTAIR | type IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | object type "Assembled Stair:190mm max riser 250mm going" | names: "Assembled Stair:Stair:497569", "Assembled Stair:Stair:591387", "Assembled Stair:Stair:592689" | parts: 30 IFCMEMBER, 6 IFCRAILING, 3 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          18 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:506703", "Basic Wall:Retaining - 300mm Concrete:506704", "Basic Wall:Retaining - 300mm Concrete:506705" (+15 more) | material: "Concrete, Cast In Situ" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          28 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:506707", "Basic Wall:Generic - 200mm:506708", "Basic Wall:Generic - 200mm:506709" (+25 more) | material: "Default Wall" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598211", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598215", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599611" (+4 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599612", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:603093" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:599614" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601120" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:601121", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602519" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601560" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603088", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603091", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603094" (+1 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604805" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604806" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604807" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
      IFCBUILDINGSTOREY "3 - Third Floor" | long name "3 - Third Floor" | object type "Level:8mm Head" | elevation 950.
        contains 106 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm" | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:358349" | material: "Default Floor" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          10 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 630mm-Render" | object type "Basic Wall:Generic - 630mm-Render" | names: "Basic Wall:Generic - 630mm-Render:358358", "Basic Wall:Generic - 630mm-Render:358359", "Basic Wall:Generic - 630mm-Render:358360" (+7 more) | material: constituents "Basic Wall:Generic - 630mm-Render" ("Render Material 240-240-240": "Render Material 240-240-240", "EIFS, Exterior Insulation": "EIFS, Exterior Insulation", "Concrete Masonry Units": "Concrete Masonry Units", "Render Material 240-240-240": "Render Material 240-240-240") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:396345", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:423940" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          5 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:397801", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:423938", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:424376" (+2 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423288", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:598219", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:598220" (+3 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423939", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:424375", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:602529" (+5 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Interior - Blockwork 190" | object type "Basic Wall:Interior - Blockwork 190" | names: "Basic Wall:Interior - Blockwork 190:433281", "Basic Wall:Interior - Blockwork 190:433282" | material: constituents "Basic Wall:Interior - Blockwork 190" ("Gypsum Wall Board": "Gypsum Wall Board", "Concrete Masonry Units": "Concrete Masonry Units", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0864 x 2134mm" | object type "M_Single-Flush:0864 x 2134mm" | DOOR | names: "M_Single-Flush:0864 x 2134mm:433493" | material: constituents ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:443703" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCSTAIR | type IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | object type "Assembled Stair:190mm max riser 250mm going" | names: "Assembled Stair:Stair:497780", "Assembled Stair:Stair:591524", "Assembled Stair:Stair:592754" | parts: 30 IFCMEMBER, 6 IFCRAILING, 3 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          18 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:506715", "Basic Wall:Retaining - 300mm Concrete:506716", "Basic Wall:Retaining - 300mm Concrete:506717" (+15 more) | material: "Concrete, Cast In Situ" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          28 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:506719", "Basic Wall:Generic - 200mm:506720", "Basic Wall:Generic - 200mm:506721" (+25 more) | material: "Default Wall" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598218", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598222", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599618" (+4 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599619", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:603103" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:599621" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601126" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:601127", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602527" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601563" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603098", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603101", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603104" (+1 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604812" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604813" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604814" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
      IFCBUILDINGSTOREY "4 - Floor" | long name "4 - Floor" | object type "Level:8mm Head" | elevation 1250.
        contains 106 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm" | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:358371" | material: "Default Floor" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          10 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 630mm-Render" | object type "Basic Wall:Generic - 630mm-Render" | names: "Basic Wall:Generic - 630mm-Render:358380", "Basic Wall:Generic - 630mm-Render:358381", "Basic Wall:Generic - 630mm-Render:358382" (+7 more) | material: constituents "Basic Wall:Generic - 630mm-Render" ("Render Material 240-240-240": "Render Material 240-240-240", "EIFS, Exterior Insulation": "EIFS, Exterior Insulation", "Concrete Masonry Units": "Concrete Masonry Units", "Render Material 240-240-240": "Render Material 240-240-240") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:396348", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:423945" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          5 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:397804", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:423943", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:424380" (+2 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423291", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:598226", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:598227" (+3 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423944", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:424379", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:602537" (+5 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Interior - Blockwork 190" | object type "Basic Wall:Interior - Blockwork 190" | names: "Basic Wall:Interior - Blockwork 190:433285", "Basic Wall:Interior - Blockwork 190:433286" | material: constituents "Basic Wall:Interior - Blockwork 190" ("Gypsum Wall Board": "Gypsum Wall Board", "Concrete Masonry Units": "Concrete Masonry Units", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0864 x 2134mm" | object type "M_Single-Flush:0864 x 2134mm" | DOOR | names: "M_Single-Flush:0864 x 2134mm:433496" | material: constituents ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:443706" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          3 x IFCSTAIR | type IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | object type "Assembled Stair:190mm max riser 250mm going" | names: "Assembled Stair:Stair:497991", "Assembled Stair:Stair:591661", "Assembled Stair:Stair:592819" | parts: 30 IFCMEMBER, 6 IFCRAILING, 3 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          18 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:506727", "Basic Wall:Retaining - 300mm Concrete:506728", "Basic Wall:Retaining - 300mm Concrete:506729" (+15 more) | material: "Concrete, Cast In Situ" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          28 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:506731", "Basic Wall:Generic - 200mm:506732", "Basic Wall:Generic - 200mm:506733" (+25 more) | material: "Default Wall" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598225", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598229", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599625" (+4 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599626", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:603113" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:599628" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601132" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:601133", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602535" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601566" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603108", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603111", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603114" (+1 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604819" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604820" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604821" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
      IFCBUILDINGSTOREY "5 - Floor" | long name "5 - Floor" | object type "Level:8mm Head" | elevation 1550.
        contains 104 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm" | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:358393" | material: "Default Floor" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          10 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 630mm-Render" | object type "Basic Wall:Generic - 630mm-Render" | names: "Basic Wall:Generic - 630mm-Render:358402", "Basic Wall:Generic - 630mm-Render:358403", "Basic Wall:Generic - 630mm-Render:358404" (+7 more) | material: constituents "Basic Wall:Generic - 630mm-Render" ("Render Material 240-240-240": "Render Material 240-240-240", "EIFS, Exterior Insulation": "EIFS, Exterior Insulation", "Concrete Masonry Units": "Concrete Masonry Units", "Render Material 240-240-240": "Render Material 240-240-240") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:396351", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:423950" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          5 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:397807", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:423948", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:424384" (+2 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          6 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423294", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:598233", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:598234" (+3 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          8 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423949", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:424383", "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:602545" (+5 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:Interior - Blockwork 190" | object type "Basic Wall:Interior - Blockwork 190" | names: "Basic Wall:Interior - Blockwork 190:433289", "Basic Wall:Interior - Blockwork 190:433290" | material: constituents "Basic Wall:Interior - Blockwork 190" ("Gypsum Wall Board": "Gypsum Wall Board", "Concrete Masonry Units": "Concrete Masonry Units", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0864 x 2134mm" | object type "M_Single-Flush:0864 x 2134mm" | DOOR | names: "M_Single-Flush:0864 x 2134mm:433499" | material: constituents ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:443709" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCSTAIR | type IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | object type "Assembled Stair:190mm max riser 250mm going" | names: "Assembled Stair:Stair:498202" | parts: 10 IFCMEMBER, 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_EnvironmentalImpactIndicators, Pset_StairCommon, Pset_StairFlightCommon
          18 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:506739", "Basic Wall:Retaining - 300mm Concrete:506740", "Basic Wall:Retaining - 300mm Concrete:506741" (+15 more) | material: "Concrete, Cast In Situ" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          28 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:506743", "Basic Wall:Generic - 200mm:506744", "Basic Wall:Generic - 200mm:506745" (+25 more) | material: "Default Wall" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          7 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598232", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598236", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599632" (+4 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599633", "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:603123" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-22:Type 2:599635" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601138" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:601139", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602543" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601569" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          4 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603118", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603121", "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:603124" (+1 more) | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604826" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604827" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604828" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
      IFCBUILDINGSTOREY "6 - Floor" | long name "6 - Floor" | object type "Level:8mm Head" | elevation 1850.
        contains 31 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm" | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:358415" | material: "Default Floor" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          13 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 630mm-Render" | object type "Basic Wall:Generic - 630mm-Render" | names: "Basic Wall:Generic - 630mm-Render:358426", "Basic Wall:Generic - 630mm-Render:505187", "Basic Wall:Generic - 630mm-Render:507256" (+10 more) | material: constituents "Basic Wall:Generic - 630mm-Render" ("Render Material 240-240-240": "Render Material 240-240-240", "EIFS, Exterior Insulation": "EIFS, Exterior Insulation", "Concrete Masonry Units": "Concrete Masonry Units", "Render Material 240-240-240": "Render Material 240-240-240") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWALL | type IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | object type "Basic Wall:Retaining - 300mm Concrete" | names: "Basic Wall:Retaining - 300mm Concrete:479128", "Basic Wall:Retaining - 300mm Concrete:479665", "Basic Wall:Retaining - 300mm Concrete:506934" (+3 more) | material: "Concrete, Cast In Situ" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm" | names: "Basic Wall:Generic - 200mm:506938", "Basic Wall:Generic - 200mm:506940", "Basic Wall:Generic - 200mm:507775" | material: "Default Wall" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 300mm_Terrace" | object type "Floor:Generic 300mm_Terrace" | FLOOR | names: "Floor:Generic 300mm_Terrace:508688" | material: constituents "Floor:Generic 300mm_Terrace" ("Default Floor_Terrace": "Default Floor_Terrace", "Layer": "Default Floor") | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORTYPE "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-21:Type 2-Glass" | object type "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-21:Type 2-Glass" | DOOR | names: "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-21:Type 2-Glass:571456" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:573986" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | object type "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | names: "Jansen_Janisol-HI_inw_TL_Family-10:Type 2:574229" | material: constituents ("<Unnamed>": "<Unnamed>", "Steel, Paint Finish, Dark Gray, Matte": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Pset_EnvironmentalImpactIndicators, Pset_WindowCommon
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | DOOR | names: "M_Single-Flush:0915 x 2134mm:574353" | material: constituents ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCDOOR | type IFCDOORTYPE "M_Single-Flush:0813 x 2134mm" | object type "M_Single-Flush:0813 x 2134mm" | DOOR | names: "M_Single-Flush:0813 x 2134mm:574520" | material: constituents ("Door - Frame": "Door - Frame", "Door - Panel": "Door - Panel") | property sets: Pset_DoorCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:Plain" | object type "Compound Ceiling:Plain" | CEILING | names: "Compound Ceiling:Plain:622512" | material: constituents "Compound Ceiling:Plain" ("Metal Stud Layer": "Metal Stud Layer", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_CoveringCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCRAILING | type IFCRAILINGTYPE "Railing:Glass Panel - Bottom Fill-meier" | object type "Railing:Glass Panel - Bottom Fill-meier" | names: "Railing:Glass Panel - Bottom Fill-meier:572345" | material: constituents ("Metal - Stainless Steel,Polished": "Metal - Stainless Steel,Polished", "Glass": "Glass", "<Unnamed>": "<Unnamed>") | property sets: Pset_EnvironmentalImpactIndicators, Pset_RailingCommon
      IFCBUILDINGSTOREY "7 - Floor" | long name "7 - Floor" | object type "Level:8mm Head" | elevation 2150.
        contains 1 element
          1 x IFCROOF | object type "Basic Roof:Steel Bar Joist - Steel Deck - EPDM Membrane" | names: "Basic Roof:Steel Bar Joist - Steel Deck - EPDM Membrane:507895" | parts: 4 IFCSLAB | property sets: Pset_EnvironmentalImpactIndicators, Pset_RoofCommon

Types
  IFCSLABTYPE "Floor:Generic 300mm" | FLOOR | 8 occurrences | material: "Default Floor" | property sets: Pset_SlabCommon
  IFCWALLTYPE "Basic Wall:Retaining - 300mm Concrete" | STANDARD | 132 occurrences | property sets: Pset_WallCommon
  IFCSTAIRTYPE "Assembled Stair:190mm max riser 250mm going" | 19 occurrences | property sets: Pset_StairCommon, Pset_StairFlightCommon
  IFCWALLTYPE "Basic Wall:Garage Wall" | STANDARD | 8 occurrences | material: constituents "Basic Wall:Garage Wall" ("Asphalt, Bitumen": "Asphalt, Bitumen", "Air": "Air", "Concrete, Cast In Situ": "Concrete, Cast In Situ") | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:Generic - 200mm" | STANDARD | 181 occurrences | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:Exterior - Brick on Mtl. Stud_63cm" | STANDARD | 8 occurrences | material: constituents "Basic Wall:Exterior - Brick on Mtl. Stud_63cm" ("Brick, Common(1)": "Brick, Common(1)", "Air": "Air", "Concrete Masonry Units": "Concrete Masonry Units", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_WallCommon
  IFCDOORTYPE "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass" | DOOR | 3 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605218, Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605218:1, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCDOORTYPE "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass" | DOOR | 6 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605751, Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605751:1, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-30:Type 1" | WINDOW | 3 occurrences | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-C4_fix_TL_Family-30:Type 1:610414, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | 1 occurrence | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-C4_fix_TL_Family-10:Type 1:614611, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | 1 occurrence | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-10:Type 2:615139, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | 3 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-22:Type 2:615259, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | WINDOW | 2 occurrences | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:615403, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | WINDOW | 1 occurrence | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:615478, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-30:Type 2" | WINDOW | 5 occurrences | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-C4_fix_TL_Family-30:Type 2:615973, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCDOORTYPE "M_Single-Flush:0915 x 2134mm" | DOOR | 1 occurrence | material: constituents ("Frame/Mullion": "Door - Frame", "Panel": "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:616505, M_Single-Flush:0915 x 2134mm:616505:1, Pset_DoorCommon
  IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | 1 occurrence | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-C4_fix_TL_Family-10:Type 1:617289, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | WINDOW | 1 occurrence | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:617926, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-30:Type 2" | WINDOW | 3 occurrences | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-C4_fix_TL_Family-30:Type 2:618466, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath" | WINDOW | 1 occurrence | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:619201, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | 2 occurrences | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-C4_fix_TL_Family-10:Type 1:620536, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | 2 occurrences | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-C4_fix_TL_Family-10:Type 1:620925, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-C4_fix_TL_Family-10:Type 1" | WINDOW | 2 occurrences | material: constituents ("Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-C4_fix_TL_Family-10:Type 1:621112, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCCURTAINWALLTYPE "Curtain Wall:Storefront- meier_Garage" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCWALLTYPE "Basic Wall:Generic - 630mm-Render" | STANDARD | 63 occurrences | material: constituents "Basic Wall:Generic - 630mm-Render" ("Render Material 240-240-240": "Render Material 240-240-240", "EIFS, Exterior Insulation": "EIFS, Exterior Insulation", "Concrete Masonry Units": "Concrete Masonry Units", "Render Material 240-240-240": "Render Material 240-240-240") | property sets: Pset_WallCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | 10 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-30:Type 2:396075, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | 25 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-10:Type 2:397507, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | 30 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423067, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | 40 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423620, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWALLTYPE "Basic Wall:Interior - Blockwork 190" | STANDARD | 10 occurrences | material: constituents "Basic Wall:Interior - Blockwork 190" ("Gypsum Wall Board": "Gypsum Wall Board", "Concrete Masonry Units": "Concrete Masonry Units", "Gypsum Wall Board": "Gypsum Wall Board") | property sets: Pset_WallCommon
  IFCDOORTYPE "M_Single-Flush:0864 x 2134mm" | DOOR | 5 occurrences | material: constituents ("Frame/Mullion": "Door - Frame", "Panel": "Door - Panel") | property sets: M_Single-Flush:0864 x 2134mm:433302, M_Single-Flush:0864 x 2134mm:433302:1, Pset_DoorCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | 5 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-10:Type 2:443514, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCCURTAINWALLTYPE "Curtain Wall:Storefront- meier" | 3 occurrences | property sets: Pset_CurtainWallCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | 36 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-10:Type 2:574229, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | 10 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598911, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-22:Type 2" | WINDOW | 5 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-22:Type 2:599313, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | 5 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599725, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | 10 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-30:Type 2:599740, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | 5 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601471, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | 20 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602615, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | 5 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604423, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | 5 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604531, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-30:Type 2" | WINDOW | 5 occurrences | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604544, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCSLABTYPE "Floor:Generic 300mm_Terrace" | FLOOR | 1 occurrence | material: constituents "Floor:Generic 300mm_Terrace" ("Default Floor_Terrace": "Default Floor_Terrace", "Layer": "Default Floor") | property sets: Pset_SlabCommon
  IFCDOORTYPE "Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-21:Type 2-Glass" | DOOR | 1 occurrence | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-21:Type 2-Glass:571456, Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-21:Type 2-Glass:571456:1, Pset_DoorCommon, Pset_ManufacturerTypeInformation
  IFCWINDOWTYPE "Jansen_Janisol-HI_inw_TL_Family-10:Type 2" | WINDOW | 1 occurrence | material: constituents ("<Unnamed>": "<Unnamed>", "Frame/Mullion": "Steel, Paint Finish, Dark Gray, Matte", "Glass": "Glass") | property sets: Jansen_Janisol-HI_inw_TL_Family-10:Type 2:573986, Pset_ManufacturerTypeInformation, Pset_WindowCommon
  IFCDOORTYPE "M_Single-Flush:0915 x 2134mm" | DOOR | 1 occurrence | material: constituents ("Frame/Mullion": "Door - Frame", "Panel": "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:574353, M_Single-Flush:0915 x 2134mm:574353:1, Pset_DoorCommon
  IFCDOORTYPE "M_Single-Flush:0813 x 2134mm" | DOOR | 1 occurrence | material: constituents ("Frame/Mullion": "Door - Frame", "Panel": "Door - Panel") | property sets: M_Single-Flush:0813 x 2134mm:574520, M_Single-Flush:0813 x 2134mm:574520:1, Pset_DoorCommon
  IFCCOVERINGTYPE "Compound Ceiling:Plain" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon
  IFCRAILINGTYPE "Railing:Glass Panel - Bottom Fill-meier" | 1 occurrence | property sets: Pset_RailingCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 361 objects (229 IFCWINDOW, 132 IFCOPENINGELEMENT)
    Reference = "Type 2" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 190 objects (190 IFCMEMBER)
    Reference = "Stringer - 50mm Width" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 181 objects (181 IFCWALL)
    Reference = "Generic - 200mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 132 objects (132 IFCWALL)
    Reference = "Retaining - 300mm Concrete" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 90 objects (90 IFCMEMBER)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 63 objects (63 IFCWALL)
    Reference = "Generic - 630mm-Render" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 38 objects (38 IFCRAILING)
    Reference = "1100mm" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 32 objects (32 IFCPLATE)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 20 more contents on 140 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 8 objects (8 IFCSLAB)
    Reference = "Generic 300mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 4 objects (4 IFCSLAB)
    Reference = "Steel Bar Joist - Steel Deck - EPDM Membrane" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Generic 300mm_Terrace" (IFCLABEL)
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic 300mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 16. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Steel Bar Joist - Steel Deck - EPDM Membrane" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic 300mm_Terrace" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfWall | properties | on 181 objects (181 IFCWALL)
    Reference = "Generic - 200mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 132 objects (132 IFCWALL)
    Reference = "Retaining - 300mm Concrete" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 63 objects (63 IFCWALL)
    Reference = "Generic - 630mm-Render" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 10 objects (10 IFCWALL)
    Reference = "Interior - Blockwork 190" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 8 objects (8 IFCWALL)
    Reference = "Garage Wall" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 8 objects (8 IFCWALL)
    Reference = "Exterior - Brick on Mtl. Stud_63cm" (IFCLABEL)
  Pset_WallCommon | properties | on 181 objects (181 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 200mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 132 objects (132 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Retaining - 300mm Concrete" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 63 objects (63 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 630mm-Render" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 10 objects (10 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - Blockwork 190" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Garage Wall" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (8 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Exterior - Brick on Mtl. Stud_63cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 3.48666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0.418216711980141 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon: 4 more contents on 0 objects not shown
  Pset_OpeningElementCommon | properties | on 132 objects (132 IFCOPENINGELEMENT)
    Reference = "Type 2" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 20 objects (20 IFCOPENINGELEMENT)
    Reference = "Storefront- meier" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Storefront- meier_Garage" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 225 objects (225 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Type 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 9 objects (9 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Type 1" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Type 2" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Type 2 - Bath" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Type 1" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Type 2 - Bath" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 30 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 9 objects (9 IFCDOOR)
    FireRating = "EI 30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Type 2 - Glass" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 5 objects (5 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0864 x 2134mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireRating = "EI 30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Type 2-Glass" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0813 x 2134mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 4 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 3 type objects
    FireRating = "EI 30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_StairCommon | properties | on 13 objects (13 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 16.6666666666647 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairCommon | properties | on 3 objects (3 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 14. (IFCCOUNTMEASURE)
    NumberOfTreads = 14. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 17.8571428571429 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairCommon | properties | on 3 objects (3 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 20. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 17.5000000000018 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
  Pset_StairFlightCommon | properties | on 13 objects (13 IFCSTAIR)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 16.6666666666647 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 13 objects (13 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 18. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "50mm Tread 13mm Riser" (IFCIDENTIFIER)
    RiserHeight = 16.6666666666647 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 3 objects (3 IFCSTAIR)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 14. (IFCCOUNTMEASURE)
    NumberOfTreads = 14. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 17.8571428571429 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 3 objects (3 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 14. (IFCCOUNTMEASURE)
    NumberOfTreads = 14. (IFCCOUNTMEASURE)
    Reference = "50mm Tread 13mm Riser" (IFCIDENTIFIER)
    RiserHeight = 17.8571428571429 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 3 objects (3 IFCSTAIR)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 20. (IFCCOUNTMEASURE)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 17.5000000000018 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 3 objects (3 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 20. (IFCCOUNTMEASURE)
    NumberOfTreads = 20. (IFCCOUNTMEASURE)
    Reference = "50mm Tread 13mm Riser" (IFCIDENTIFIER)
    RiserHeight = 17.5000000000018 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtInnerSide = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 25. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 1.64041994750656 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 1 type object
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 0. (IFCCOUNTMEASURE)
    NumberOfTreads = 0. (IFCCOUNTMEASURE)
  Pset_MemberCommon | properties | on 76 objects (76 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stringer - 50mm Width" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 26 objects (26 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 293.999999999993 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 20 objects (20 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 122.5 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 16 objects (16 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 288.833333333327 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 14 objects (14 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stringer - 50mm Width" (IFCIDENTIFIER)
    Slope = 41.9499108990975 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 13 objects (13 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stringer - 50mm Width" (IFCIDENTIFIER)
    Slope = 20.8542255359278 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 12 objects (12 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Stringer - 50mm Width" (IFCIDENTIFIER)
    Slope = 26.6343109992907 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_MemberCommon | properties | on 12 objects (12 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "50 x 150mm" (IFCIDENTIFIER)
    Span = 122.5 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon: 36 more contents on 91 objects not shown
  Pset_CurtainWallCommon | properties | on 3 objects (3 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Storefront- meier" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Storefront- meier_Garage" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 2 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_PlateCommon | properties | on 20 objects (20 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 12 objects (12 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 1 object (1 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Solid" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Steel Bar Joist - Steel Deck - EPDM Membrane" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Plain" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0.549915397631134 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RailingCommon | properties | on 38 objects (38 IFCRAILING)
    Height = 110. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100mm" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 90. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Glass Panel - Bottom Fill-meier" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 9 objects (9 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "8mm Head" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 9 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)
  Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605218 | predefined | on 1 type object
  Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605218:1 | predefined | on 1 type object
  Pset_ManufacturerTypeInformation | properties | on 33 type objects
    Manufacturer = "Jansen AG" (IFCLABEL)
  Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605751 | predefined | on 1 type object
  Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-30:Type 2 - Glass:605751:1 | predefined | on 1 type object
  Jansen_Janisol-C4_fix_TL_Family-30:Type 1:610414 | predefined | on 1 type object
  Jansen_Janisol-C4_fix_TL_Family-10:Type 1:614611 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-10:Type 2:615139 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-22:Type 2:615259 | predefined | on 1 type object
  Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:615403 | predefined | on 1 type object
  Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:615478 | predefined | on 1 type object
  Jansen_Janisol-C4_fix_TL_Family-30:Type 2:615973 | predefined | on 1 type object
  M_Single-Flush:0915 x 2134mm:616505 | predefined | on 1 type object
  M_Single-Flush:0915 x 2134mm:616505:1 | predefined | on 1 type object
  Jansen_Janisol-C4_fix_TL_Family-10:Type 1:617289 | predefined | on 1 type object
  Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:617926 | predefined | on 1 type object
  Jansen_Janisol-C4_fix_TL_Family-30:Type 2:618466 | predefined | on 1 type object
  Jansen_Janisol-Steel_fix_TL_Family-10:Type 2 - Bath:619201 | predefined | on 1 type object
  Jansen_Janisol-C4_fix_TL_Family-10:Type 1:620536 | predefined | on 1 type object
  Jansen_Janisol-C4_fix_TL_Family-10:Type 1:620925 | predefined | on 1 type object
  Jansen_Janisol-C4_fix_TL_Family-10:Type 1:621112 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-30:Type 2:396075 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-10:Type 2:397507 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423067 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-22:Type 2:423620 | predefined | on 1 type object
  M_Single-Flush:0864 x 2134mm:433302 | predefined | on 1 type object
  M_Single-Flush:0864 x 2134mm:433302:1 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-10:Type 2:443514 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-10:Type 2:574229 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-10:Type 2:598911 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-22:Type 2:599313 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-10:Type 2:599725 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-30:Type 2:599740 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-10:Type 2:601471 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-30:Type 2:602615 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604423 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604531 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-30:Type 2:604544 | predefined | on 1 type object
  Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-21:Type 2-Glass:571456 | predefined | on 1 type object
  Jansen_Janisol-2-EI30-70mm-Door_inw_TL_Family-21:Type 2-Glass:571456:1 | predefined | on 1 type object
  Jansen_Janisol-HI_inw_TL_Family-10:Type 2:573986 | predefined | on 1 type object
  M_Single-Flush:0915 x 2134mm:574353 | predefined | on 1 type object
  M_Single-Flush:0915 x 2134mm:574353:1 | predefined | on 1 type object
  M_Single-Flush:0813 x 2134mm:574520 | predefined | on 1 type object
  M_Single-Flush:0813 x 2134mm:574520:1 | predefined | on 1 type object